|  |  |
| --- | --- |
| Title | Super Clean |
| Product Category: | Degreasers Water Based |
| Description: | SUPER CLEAN is a water-based solvent for cleaning walls, floors, machinery, vinyl and carpets, removing grease, oil, dirt, grime, carbon, soot, ink, food and most other soils. |
| Picture: |  |
| Applications: | Industrial Sites  Professional Workers  Consumer Uses |
| Technical Data: | |  |  | | --- | --- | | **Base Units:** | Litres | | **Form:** | Liquid | | **Colour:** | Various | | **Odour:** | Sweet |  |  |  | | --- | --- | | **Solubility:** |  | | **Solubility in water:** | Soluble | | **Specific Gravity (20 °C):** | 1.02 | | **Relative Vapour Density (air=1):** | >1 | | **Boiling Point/Range (°C):** | >100 | | **pH:** | 10.5-11.5 | | **Evaporation Rate (n-Butyl acetate=1):** | <1 | |
| Personal Protective Equipment: | GLOVES, SAFETY GLASSES |
| Directions for use: | Use diluted 20 to 1 for most cleaning jobs. Corrosion inhibitors included to give safe cleaning on metal surfaces.WALLS: Mix 1:12 and spray on holding sponge underneath. On larger areas, clean from bottom up.WAX REMOVALMix 1:10 with hot water, apply to floor generously, wait five minutes then scrub with nylon pad or scrub brush.VINYL UPHOLSTERYMix 1:8 in sprayer. Spray on. After two minutes wipe with sponge.DEGREASINGMix up to 1:10 and apply. Allow four minutes for penetration. Wash with hose or power sprayer.WHITEWALLSMix 1:6 and spray on. Wipe with a rag and rinse with hose.COIL CLEANINGApply only when unit is not running. Dilute 1 part product to 5 parts water and apply to coil. Repeat if necessary . No rinsingrequired. |
| Item # / Pack Size: | |  |  |  | | --- | --- | --- | | **Synonyms** | **Product Code** | **Bar Code** | | Super Clean 1000Ltr POD |  | 16-02-1125-1000 | | Super Clean 200L |  | 16-02-1125-200 | | Super Clean 20L |  | 16-02-1125-20 | | Super Clean 25L |  | 16-02-1125-25 | | Super Clean 5L |  | 16-02-1125-5 | | Super Clean Bulk |  | 31-05-0558 | |
| Supplier: | |  |  | | --- | --- | | **Name** | Minehan Agencies Pty Ltd | | **Company number** | 21 010 895 100 | | **Address** | 29 Camuglia Street, Garbutt,  Townsville, QLD 4814  Australia | | **Telephone** | 07 4774 4626 | | **Fax** | 07 4774 4616 | | **Email** | inquiry@minehanagencies.com.au | | **Website URL** | www.minehanagencies.com.au | |